[image: ]This has been provided directly from the Watersports Centre yachting chief instructor, and has not been edited by Formula Sailing in any way.

 This is used in conjunction with their operating procedures, as seen here: https://sotonac.sharepoint.com/teams/SportWellbeing/SitePages/Watersports-NOP-Yacht-NOP.aspx
Again, this has not been amended by us in any way, and we would not deviate from the Watersports centres risk assessment recommendations or standard operating procedures without specifically consulting them. 
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Yacht Use

Hazards Who & How Harmed What We Are Doing Risk Rating

Berthing the yacht Collision with other boats or pontoon - Students, staff, public onboard: other boats and people | Skippers observed for competence: fenders on boat. Roaming fender advised; boat insured. Low

Bost breakdown at sea Stranded, hungerfthrst - Students, staff, public onboard VHE radio; anchor: Sea Start membership for assistance. Low

Boat sinking or mayday with electrical failure Unable to contact help during distress - Students, staf, public onboard Life raft and jackets onboard: flares available: portable handheld VHF with DSC button Medium

Cold exposure in winter Hypothermia - Students, staff, public onboard Pre-tip bricfing on clothing: recommend hat. gloves, thermals, Layers Low

Electr Electric shack or fire - Students, staf. public onbosrd Multple breakers: labelled wiring; fuses to prevent overheating; galvanic isolator fitted and earthed. Medium

Risk of drawning if peaple enter the water - Students, staf, public anbx Bost inspected to CAT 2 level; fe jackets with Lights; Ufe raft onbosrd: mandatory lfe jacket use on deck: skipper emergency brisfing. High

rom gas oven system Explosion or fire onbosrd - Students, staf, public on (Gas system isolatable in two places: bottles stored in vented locker; gas sniffer alarm operational and tested regularly, High

 fumes from inbosrd engine Fire or choking from fumes - Students, staf, public on Engine stored in sealed compartment: diesel engine reduces explosion risk; annual servicing: gas sniffe alarm tested regularly Medium

it by boom or mainshest track Serious head injury - Students, staff, public onboard briefs crew: safe seating positions: lfe High

Lack of knowledge of boat systems nability to operate safely - Students, staff, public onboar hensive notes onboard: skipper induction before use. Low

Rigging entrapment Person trapped and dragged overboard - Students, staff, public onboard briefing on safe areas: bolt croppers and hacksaw onboard for emergency cutting, Medium

Running aground in shallow a Boat stranded; keel damage - Students, saff, public onboard Depth sounder: chart pltter: charts ont aware of tidesinavigation Low

Sailing in very windy conditions Equipment faiure, seasickness, injury. Students, staf, public onboard AL34 Knots of mean wind speed return yacht to 3 port refuge. Low

Sea cock failure: Boat sinking, loss of ife - Students, staf, public onboard Coding and pre-purchase surveys: regular checks; wooden bungs near sea cocks: spare bungs onboard: two manual and one electric bilge pump operationa Medium

Using gas hobs Burns from spillage - Students, staff public onboard. Assess sea state before boiling: gimballed cooker with kettle holder Medium

ing winches Finger/hand injury - Students, staff, public onboard Training before use: supervision for beginners Medium

Walking around boat at Head injury. fals - Students, staff, public onboard Handrails: lights: guard rail: harness lines available High

Walking around wet boat or companionway steps | Slips and falls - Students, staf, public onboard Safety briefing: proper footwesr; handrails; ant-slp tread on steps. Low
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